> # Mounting Your DVD

> This section provides DVD mounting instructions for your SequeLink platform.

> ### Windows

> The supported Windows platforms provide the system option AutoRun for DVDs as a default feature. If enabled, the Product Setup starts immediately when you insert the DVD in the DVD-ROM drive.

> If AutoRun for DVDs is disabled, or you are mounting the DVD on a network drive:

> 1. Insert the DVD into the DVD-ROM drive (for a local driver, this typically is drive D). If the DVD-ROM drive is on a network, mount the DVD and create a mapping to the DVD-ROM drive.
> 2. To view the contents of the DVD, double-click the DVD-ROM drive icon in the My Computer window.

> ### UNIX

> Sun Solaris

> By default, the DVD-ROM drive mounts automatically when you insert the DVD. The other supported UNIX platforms do not automatically mount the DVD by default. If your workstation is not configured to mount a DVD automatically, you must enter the command for mounting the DVD.

> HP-UX

>     # /usr/sbin/pfs_mountd&
>     # /usr/sbin/pfsd&
>     # pfs_mount -o xlat=unix /dev/rdsk/deviceName /dvdrom

> where deviceName is the device name assigned to your DVD-ROM drive. The device name can be found using the HP-UX tool sam. When installation is complete, unmount the DVD-ROM with the command:

>     # /usr/sbin/pfs_umount /dvdrom

> For example, if the device name for your DVD-ROM drive is /dev/rdsk/c0t4d0, and you want to mount it over the directory /dvdrom, you would enter the following command:

>     # pfs_mount -o xlat=unix /dev/rdsk/c0t4d0 /dvdrom

> IBM-AIX

>     mount -r -v dvdrfs /dev/deviceName /dvdrom

> where `deviceName` is the device name assigned to your DVD-ROM drive. The device name can be found using the AIX tool smit.

> For example:

>     mount -r -v dvdrfs /dev/dvd0 /dvdrom

> Linux

>     # mount -r -t iso9660 /dev/deviceName /mnt/dvdrom

> where `deviceName` is the device name assigned to your DVD-ROM drive.