> # Operator Interface Messages

> This section contains z/OS log messages generated by VAICOPRI, which handles operator interface processing.

> VAIC033I | Occurs when trying to execute LOGR PRINT.
> | Severity: | Information
> | Explanation: | If the VAILOGP is sent to SYSOUT, it cannot be printed with SequeLink commands.
> | System action: | The VAILOGP is not printed.
> | User response: | Use the JES commands to print VAILOGP.
> VAIC100I | Unknown operator command type (not modify or stop) - Probable internal error.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an unknown command type from an operator's console.
> | System action: | Processing continues; the command is ignored.
> | User response: | This is an internal error. Report this message to DataDirect Technologies technical support.
> VAIC101T | Command in: command.
> | Severity: | Trace
> | Explanation: | The operator interface component of the server system received the specified command from the operator's console.
> | System action: | Not applicable.
> | User response: | None.
> VAIC102I | Parse failure on operator command ... format expected is: ROUTID VERB F1=..fld.. F2=..fld.. etc.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an incorrect command from the operator's console. The command received did not follow the expected format.
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC103I | Command indicated an unsupported ROUTE ID.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an incorrect command from the operator's console. The command received contained an invalid route or component ID.
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC104I | Command indicated an unsupported verb verbname.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an incorrect command from the operator's console. The command contained an invalid verb.
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC105I | Required parameter field missing from command.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an incorrect command from the operator's console. The command that was entered had a required field missing.
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC106I | Unknown parameter field in command.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an incorrect command from the operator's console. The command that was entered included an unknown field.
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC107I | Extraneous parameter name in command.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an incorrect command from the operator's console. The command that was entered included an unknown parameter (parameter name).
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC108I | Command parameter field exceeds maximum length.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received an incorrect command from the operator's console. The command that was entered included a parameter field with a length which exceeded the maximum allowed.
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC109T | ** Command accepted for routing (CONSOLE ID = ID).
> | Severity: | Trace
> | Explanation: | The operator interface component of the server system received a command from the operator's console. The command passed all validity checking by the operator interface component. The command originated from the console identified by the stated console ID.
> | System action: | Not applicable.
> | User response: | None.
> VAIC110I | Unrecognized parameter field(s) in command.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system received a command from the operator's console. The command that was entered included an unknown parameter.
> | System action: | The entered command is ignored.
> | User response: | Check the syntax of the command and reenter the correct command.
> VAIC111S | Not able to assign command buffer - internal error.
> | Severity: | Severe
> | Explanation: | The operator interface component of the server system received a command from the operator's console. The operator interface (VAICOPRI) was unable to assign a storage buffer to the command.
> | System action: | The entered command is ignored.
> | User response: | This is an internal error. Report this message to DataDirect Technologies technical support.
> VAIC113F | VAICOPRI - Error loading VAICOPRI-VAICCMDS - Terminating.
> | Severity: | Fatal
> | Explanation: | The operator interface component of the server system failed in its attempt to load one of its external routines.
> | System action: | The server system abends with an abend code of U146.
> | User response: | Verify the integrity of the server's executable library. Recover the library from a backup tape, if necessary. Contact DataDirect Technologies technical support for assistance, if you are unable to correct the library failure.
> VAIC114S | VAICOPRI -TACB search for COMPONENT component ID failed - command ignored.
> | Severity: | Severe
> | Explanation: | The operator interface component of the server system received a command from the operator's console. The command contained the stated route or component ID, but the system could not locate a corresponding component.
> | System action: | The entered command is ignored.
> | User response: | Ensure that the component ID specified in the command is currently enabled within your Server system. If the specified component is enabled and you still receive this message, contact DataDirect Technologies technical support.
> VAIC115I | Operator interface initialization completed OK.
> | Severity: | Information
> | Explanation: | The operator interface component of the server system successfully completed initialization.
> | System action: | The operator interface component will accept control commands.
> | User response: | None.
> VAIC117E | You are not authorized to issue command.
> | Severity: | Error
> | Explanation: | You have attempted to issue an operator command for which you have inadequate authorization.
> | System action: | The command is ignored.
> | User response: | If necessary, ask your system administrator to update your security access. Refer to the SequeLink Administrator's Guide for information about different types of security access.
> VAIC118I | CommandPrefix character(s) missing or blank.
> | Severity: | Information
> | Explanation: | Specifying a non-blank CRC causes the SSI to be activated. This message informs you that the SSI will be inactive because the CommandPrefix character (CP) was either omitted from the DataModel or specified as blank.
> | System action: | The SequeLink for z/OS SSI is not activated.
> | User response: | The default CP is blank, meaning the SSI will not be activated if the CP is not explicitly specified in the DataModel. If the SSI is to be activated, specify a non-blank DataModel CP value and restart SequeLink for z/OS.
> VAIC119I | SSID missing/blank or has an invalid Length.
> | Severity: | Information
> | Explanation: | The SequeLink for z/OS subsystem ID (SSID) was either omitted from SYSINI or specified as blank.
> | System action: | The SequeLink for z/OS SSI is not activated.
> | User response: | If the SSI is to be activated, correct the SYSINI SSID value and restart SequeLink for z/OS.
> VAIC120E | SSI SSCT construction failure.
> | Severity: | Error
> | Explanation: | During initialization of the SequeLink for z/OS SSI, an error occurred attempting to construct the SSCT structure. The most probable reason is CSA space could not be obtained.
> | System action: | The SequeLink for z/OS SSI is not activated.
> | User response: | Report this error to DataDirect Technologies technical support.
> VAIC121E | SSI activation failure.
> | Severity: | Error
> | Explanation: | Activation of the SequeLink for z/OS SSI was unsuccessful.
> | System action: | The SequeLink for z/OS SSI is not activated.
> | User response: | This message is usually preceded by either VAIC124E or VAIC126E; check that message for the appropriate action. Otherwise, contact DataDirect Technologies technical support.
> VAIC122I | CommandPrefix(pppppppp) used for SubSystem(ssss).
> | Severity: | Information
> | Explanation: | Messages showing information about Subsystem Interface setup, where: ssss`-` Is the Subsystem Name pppppppp`-` Is the CommandPrefix
> | System action: | Not applicable.
> | User response: | None.
> VAIC123E | SSI (ssss) is in use by another SequeLink for z/OS.
> | Severity: | Error
> | Explanation: | SequeLink for z/OS SSI initialization detected an active SSI (SSid) for the SSID specified in the SYSINI. SequeLink Server starts up normally, but the command recognition character cannot be used to issue SequeLink commands. Change the SYSINI and use an available SSID.
> | System action: | None.
> | User response: | None.
> VAIC124E | SSI(ssss) not associated with SequeLink MVS.
> | Severity: | Error
> | Explanation: | SubsystemName ssss already in use by another Subsystem.
> | System action: | None.
> | User response: | Choose another SubsystemName for use by SequeLink.
> VAIC126E | Invalid CommandPrefix(pppp) for Subsystem(ssss), rc=xx reason=yy.
> | Severity: | Error
> | Explanation: | SubsystemName ssss already in use by another Subsystem.
> | System action: | None.
> | User response: | Probably pppp is a subset of an existing CommandPrefix. Use MVS 'DISPLAY OPDATA' command to check this. Also, see the z/OS CPF macro for rc and reason codes.